**Corbetti Geothermal, Diesel Generators for water supply system**

The works involves the complete design, manufacture, supply, transportation to Addis Ababa of four (4) sets of diesel generators and spare parts for water supply system. The gen set load is of two types, a single gen set supplying one borehole pump and a single Gen Set supplying two booster pumps. The gen Sets will be installed at an altitude of 1900 (6.200 ft) m above sea level. The estimated rated motor power is 45 to 75 kW at 380 V rated voltage and 85 – 135 A rated current.

Tender documents will be delivered by email and shall Interested bidders contact [elin@mannvit.is](mailto:elin@mannvit.is) or [Helgi@CorbettiGeothermal.com](mailto:Helgi@CorbettiGeothermal.com) to receive the RFP.

Tenders shall be submitted in email to [elin@mannvit.is](mailto:elin@mannvit.is), [Helgi@CorbettiGeothermal.com](mailto:Helgi@CorbettiGeothermal.com) and [Dawit@CorbettiGeothermal.com](mailto:Dawit@CorbettiGeothermal.com)

**Important Dates & Other Details**

Open procedure - Yes

Inquiry deadline: 7th May, 2018

Answering Deadline: 9th May, 2018

Tenders will be opened at: 14th May, 2018 time: 14:30

Place of opening Tenders: Haimi Building, 2nd Floor, Namibia Street, Bole Sub City, Kebele 03/05 - Addis Ababa, Ethiopia

The Tenders shall be valid for 8 weeks after opening day.

Delivery deadline: 14th May 2018 time: 14:00